**Automated Surveillance using Background Subtraction and Shape Analysis**

Final Report for CS39440 Major Project

*Author*: Alexander Shaun O’Donnell ([alo14@aber.ac.uk](mailto:alo14@aber.ac.uk))

*Supervisor*: Bernie Tiddeman (bpt@aber.ac.uk)

16th April 2016

Version 1.0 (Draft)

This report is submitted as partial fulfilment of a BSc degree in  
Computer Science (Inc Integrated Industrial and Professional Training) (G401)

Department of Computer Science

Aberystwyth University

Aberystwyth

Ceredigion

SY23 3DB

Wales, UK

**Declaration of originality**

I confirm that:

* This submission is my own work, except where clearly indicated.
* I understand that there are severe penalties for Unacceptable Academic Practice, which can lead to loss of marks or even the withholding of a degree.
* I have read the regulations on Unacceptable Academic Practice from the University’s Academic Quality and Records Office (AQRO) and the relevant sections of the current Student Handbook of the Department of Computer Science.
* In submitting this work I understand and agree to abide by the University’s regulations governing these issues.

Name Alexander Shaun O’Donnell



Date 16/04/2017

**Consent to share this work**

By including my name below, I hereby agree to this dissertation being made available to other students and academic staff of the Aberystwyth Computer Science Department.

Name Alexander Shaun O’Donnell



Date 16/04/2017

**Acknowledgements**

I am grateful to…

I’d like to thank…

**Abstract**

Computer vision and image interpretation are evolving topics in the world of technology. Many institutions have invested in this field of research for security solutions, as technologies such as facial recognition, object placement and pedestrian detection can provide potential safety nets to the challenges they face. The rise of automation technologies is reducing human error, which is something a high-risk field such as security could do without. This project looks at pedestrian detection/tracking, the idea that a program could take up the role of monitoring live CCTV footage and keep a record of pedestrians and other movements. We can achieve this by using what is known as a classifier, an algorithm that can lead software to make categorical decisions. By providing examples of how pedestrians may appear in a video, the classifier can distinguish between what is and what isn’t a person. Assuming the cameras used in the videos are static, moving objects can be separated from a non-moving environment using background subtraction. Combining these tools, we can extract large moving objects from video footage and use the classifier to see whether the object is a person or not. Rather than having a police officer go through hours of CCTV footage, this program can view the video instead, recording any passenger or movement that occurred with a timestamp of when it happened.

**Contents**

1. Background, Analysis & Process 7

1.1. Background 7

1.1.1. Security and Automation 7

1.1.2. Detection through Vision 7

1.1.3. Pedestrian Detection 8

1.1.4. Motion Detection 9

1.2. Analysis 11

1.2.1. Objectives 11

1.2.2. Datasets and Frameworks 12

1.2.3. Motion Detection Choice 13

1.2.4. Feature Selection and Classification 13

1.2.5. Record Log 14

1.2.6. Issues 14

1.2.7. Security 15

1.3. Process 15

1.3.1. Methodology 15

1.3.2. Support tools 15

2. Design 17

2.1. Overall Architecture 17

2.2. Features List 17

2.2.1. Getting training data 17

2.2.2. Outline shape contours 17

2.2.3. Build pedestrian model 17

2.2.4. Train pedestrian finder 17

2.2.5. Run the input video 17

2.2.6. Apply BGS 17

2.2.7. Display source video and BGS 17

2.2.8. Classify shape 17

2.2.9. Record findings 17

2.3. Pedestrian model sub features 17

2.3.1. Search for the head 17

2.4. Other Relevant Sections 17

3. Implementation 18

4. Testing 19

4.1. Overall Approach to Testing 19

4.2. Automated Testing 19

4.2.1. Unit Tests 19

4.2.2. User Interface Testing 19

4.2.3. Stress Testing 19

4.2.4. Other Types of Testing 19

4.3. Integration Testing 19

4.4. User Testing 19

5. Critical Evaluation 20

6. Appendices 21

A. Third-Party Code and Libraries 21

B. Ethics Submission 22

C. Code Samples 23

Annotated Bibliography 24

# Background, Analysis & Process

## Background

### Security and Automation

As an interdisciplinary field, computer vision has provided many solutions to security. From facial recognition for matching perpetrators to crowd analysis for tackling gang culture and hooliganism, it synergises well with high risk environments. Originating in academic environments, computer vision made its way into the world of security as early as 2001. Police in Tampa, Florida used facial recognition software during the Super Bowl XXXV in January 2001 to detect known criminals and terrorists attempting to attend the event. The software, known as “FaceIt” was developed by Identix and managed to find 19 people with pending arrest warrants [1].

Computer Vision is an abstract topic, the idea of getting a system to understand what is being depicted in an image is particularly useful for security. Many institutions have researched this field as it can provide solutions to some of the challenges faced by the industry. For example, in 2015 the Ministry of Defence (MoD) cooperated with QinetiQ to develop middleware software architecture that would be used alongside sophisticated sensing equipment to perform detection and behaviour classification in a specified area [2].

A typical surveillance setup would involve a security guard or member of law enforcement observing several cameras. These cameras are usually static, where a single camera will maintain the same viewing angle for its duration. This results in institutions investing in many cameras to cover all angles of a premises, and can be straining on the employee tasked to observe them all. This is amplified in isolated or rural environments, where cameras may only observe a small number of pedestrians every hour leading to fatigue and thus an increase in human error. Previous studies have coined the term ‘boredom factor’, where an observer’s levels of concentration degrade over time from viewing the same monotonous feeds for long hour shifts [3].

Part of the job for police officers is to review pre-recorded CCTV footage recorded for potential evidence, with footage lengths ranging from minutes to days. In 2016 CCTV operators from the Suffolk Constabulary and the Metropolitan Police observed more than 1100 hours CCTV footage in the search for a missing person [4]. The hours spent on this particular case involved detection rather than recognition, as they do not include identifying the individuals found. The ability to automate this process would save time, resources and manpower that could be better spent in agencies such as these. It is vital that our law enforcement adapts and becomes more efficient at retrieving and storing information for the sake of the victims and our privacy. To automate the process of collecting timestamps of people appearing in videos, we can look no further than the field of pedestrian detection.

### Detection through Vision

Pedestrian detection is a sub topic of object detection, and has become a fundamental task in video surveillance. The ability to detect and track a human provides great support for reducing trespassers in restricted areas. Typical detection applications in computer vision rely on a classifying algorithm, and some form of machine learning with training/testing phases.

The training phase provides the program with examples of how the object it’s looking for may appear (a person in our case). These examples come in the form of a dataset, a collection of images representing the object to detect. Some datasets include what is known as negative examples, images which either represent something different or don’t include the object altogether. This opens up the classifier to different categories so it can overcome common appearances that interfere with its decision making. For example, including images of cars or animals would help the program differentiate pedestrians from other objects relevant to the environment.

There are a wide range of methods for detecting and classifying objects, many of which are based on the Viola-Jones object detection framework. Although the framework was initially intended for face detection, there have been adaptations to suit pedestrian detection. Viola-Jones is also referred to as a ‘Haar Cascade Algorithm’ since the framework relies on Haar-like feature selection and cascade architecture for classification.

Haar-like feature works by looking at the difference in the sum of the pixel intensities in specific regions of the image. These rectangular regions are positioned relative to a boundary box, this window is scanned across the image to find intensity changes that appear within the regions. Since faces share common appearances such as changes in colour between the eyes and cheek, it is worth positioning the rectangles in the upper areas of the bounding box. In the Fig 1, the rectangle in the middle compares the difference in colour between the eyes/eye brows and the nose/cheeks. The rectangle on the right compares the changes in colour for either side of the nose bridge, assuming that these areas will appear darker.



Fig 1. Rectangular regions used for detecting eyes during face detection. (Source: <http://docs.opencv.org/trunk/d7/d8b/tutorial_py_face_detection.html> )

By applying feature finding techniques to a training set, the program can get a better idea of how faces may appear, as well as a threshold for distinguishing faces from non-faces. There will always be a false positive risk with detection algorithms, for example pareidolic images without a face, that happen to have darker regions where the eyes would be could still possibly be classified as a face. Which is why many classifiers take in a threshold or a Gaussian of intensity values to differentiate faces from noisy images.

Viola-Jones relies on cascade classification, a combination of many classifiers in order of complexity. Each classifier is trained on the same sample, if one classifier rejects the image than the classification breaks out, reducing the processing time so it can search the next sample. This also enables the cascade to focus on more promising regions in the image that are more likely to contain the features, increasing the detection rates as the search space is reduced [5].

### Pedestrian Detection

Pedestrian detection can be achieved using Haar-like features, changes in pixel intensity in simple environments can be seen on people as well as faces. The rectangles can be rearranged within the search window, looking for intensity changes around the head, hands and feet. This assumes the appearance of the person stands out from the environment or that an appropriate threshold is used.

Local Haar features can be combined to build a pedestrian model. Recently, pedestrian detection was achieved by constructing square body shape models from gradient magnitudes and colour channels (Zhang et al, 2014) [6]. Their statistical model takes in images and computes an average edge map of the sample. The resulting edge map is divided into cells, which construct the square regions that make up the body. Their body model is divided into three sections, the head, torso and legs. This is useful as it reduces the search space for features, since it would be safe to assume the feet features always appear below the torso. The core of their project uses multi-channel descriptors for the cells for more information at a local level, and AdaBoost classification, similar to that of Viola-Jones.

Pedestrian detection has seen progress outside of Haar Cascade in recent decades, the increase in publicly available datasets and frameworks has made computer vision more accessible. 2005 saw Dalal & Triggs introduce the histogram of gradients (HOG) feature descriptor which became a landmark for human detection. The descriptor computes the gradients of the input image, and then dividing it into cells. For each cell, a histogram is made of the edge orientations, with the most common orientation representing the direction of the edge within that cell. Linking these orientations together forms a representation of the shape, and exceeds at handling rotations and different human poses [7].




Fig 2. Visual representation of cell directions derived from the HOG feature descriptor. (Source: <http://www.learnopencv.com/histogram-of-oriented-gradients/> )

Detectors such as these begin to use more information from the given images to handle variation in clothing and lighting. These methods demonstrate how effective it is to reduce feature complexity by summarising them into simpler regions. Ultimately making pedestrian detection more adjusted to variations in a person’s appearance. These pedestrian detectors rely on deriving shapes from edges, colour and orientation, we can also derive shape from motion.

### Motion Detection

Points of interest in an image or video are usually moving, with CCTV cameras for example interesting frames usually involve people entering and leaving the perspective. It worth considering the options that motion detection algorithms provide regarding pedestrian detection. As Haar has shown, reducing the search space to regions of interest lead to more computationally efficient programs. Reducing the search space of our pedestrian detector to moving objects could increase its optimisation, as well as reduce the amount of background interference.

One method for detecting motion is background subtraction(BGS), which involves taking the parts of a video that aren’t moving and ignoring them. The moving/non-moving parts in the video are separated, the moving parts are extracted to what is known as the foreground mask. BGS requires a static camera, since it would fail to distinguish anything from a frame where everything is moving. Fortunately, many surveillance systems use on static cameras, and rely on using many cameras to cover key areas of the perimeter. A simple BGS formula would simply subtract the change in pixel intensities between the current frame and the previous frame.



Fig 3. BGS being run on the CAVIAR dataset.

You also need to consider lighting and animated background features. An environment that has a constant shift in lighting effects may return a poor foreground mask. A BGS camera setup of a road with street lamps would struggle with lighting changes as well as shadows emanating from objects at certain angles. Meanwhile a coastal area would have light reflecting of the waves further distorting the mask. Considering not all moving feature of an image are of interest, animated background areas may cause issues. Things such as waves, flags, vehicles and small animals would all appear on the foreground mask if no filtering process was present. Many of these issues can be filtered or reduced through parameters and noise cancelling.

To determine whether a pixel is counted as moving, more advanced methods rely on a ‘history’ parameter. This parameter is usually arbitrary, if something moves in that pixel, the history represents the number of time/frames that pass before the pixel is counted as static. Reducing the history value could tackle the lighting issue, depending how slow the change in lighting is. If the foreground mask is only registering quicker movements, than slower changes in lighting could be ignored.

For the non-interest animated background features, a threshold can be introduced. This threshold would define how much the pixel intensity needs to change between frames before the pixel can be seen as ‘moving’. Through thresholding the foreground mask, smaller movements within the picture such as shadows can be ignored. Modern BGS functions can adapt this threshold to deal with long term changes within the background, such as objects being placed in the scene and day/night cycles.

Another way of detecting motion is using optical flow. Similar to the visualisation in Fig 2, regions within an image are said to have a direction. An optical flow method works out the direction of travel for each cell of an image. Optical flow methods are useful as they can show the strength of the direction as well as it’s orientation, which gives information on how fast the motion is. Optical flow is more suited to dynamic environments, since it can quickly adapt if the camera moves.

One of the biggest issues in computer vision is tackling noise. Image noise is unwanted side effects that occur when visualising a computer vision algorithm, and has a wide range of forms and causes. Examples of noise include speckles, film grain and static, which all add extraneous information. The most common cause of noise is the use of low resolution cameras, a lower number of pixels means that noisy areas will have a greater effect on the overall image quality. It is important to consider noise reduction techniques as clearer images which produce more obvious features and shapes, making easier for algorithms to find them.

Erosion morphology can be used to reduce the amount of speckle noise in BGS. Assume it is being applied to binary foreground mask, where pixel greyscale values are either 0 (non-moving) or 255 (moving). Erosion uses a structuring element to determine which of the current pixel’s neighbours must be 255, for its value to still be 255 after processing. Erosion examines the neighbouring pixels of a selected pixel, if the current pixel has at least one neighbour with a value of 0, the pixel’s value becomes 0.




Fig 4. Applying a 3x3 structuring element across an image, a 255 pixel (white) must have the pixels adjacent to it be 255 to survive erosion.

## Analysis

### Objectives

The objectives for the project can be summarised as the following:

* Create a pedestrian detection system that can highlight pedestrians in images
* Run pedestrian detection on source videos
* Locate localised features within shapes to build an overall skeleton model
* Train the system on ground truth data
* Have a system that can differentiate between pedestrians and noise
* Record detected pedestrians in a log

The aim of this project was to automate the process of detecting and tracking pedestrians within a video. From loading the project, the user would be able to select a video to analyse, gaining live feedback of the programs interpretation of what is going on. An ideal project would have a menu or interface, where the user can input threshold values and see their effects in real time. To have pedestrian detection run on live footage would be beneficial, where it could track a livestream through screen capture functionality. However, this required extensive coding which may not be possible during the timeframe. Since the primary aim of this project is successful pedestrian detection, running it on pre-recorded videos may be suitable enough.

The program needed some live feedback, whatever the pedestrian detector is reading should be displayed alongside the source video. This would make the project more engaging if the user could at least visualise the readings while the videos are being played.

It needed some interpretation or knowledge of what it’s looking at, so it can distinguish pedestrians from noise. This would require the code to implement a basic training stage so it can construct its own idea of what a pedestrian looks like. It should return accurate cut outs of pedestrians that appear in the video, rather than printing out every single entire frame as this would show it has poor reliability.

The program must be able to somehow document the pedestrians/features it has witnessed throughout the video. Rather than having security officers go through hours and hours of footage looking for people, the program will have a full list of the pedestrians that appeared with timestamps. The record log will contain information such as the time in the video, cut outs of the pedestrian alongside the programs interpretation of their shape, and a verdict on whether the program believes it was a pedestrian or something else. This log wouldn’t need to be too complex, as long as it is clear which pedestrians appeared at what time.

The project was done in C++, my industrial year gave me experience with C, however there are computer vision related frameworks available in C++. An object-oriented language such as C++ provides better class structure and data management than C which relies heavily on structs.

### Datasets and Frameworks

With the amount of freely available datasets and open source frameworks, its ideal to use proven computer vision functions/datasets for this project. An ideal dataset would provide video files of static cameras observing realistic behaviours and environments. Better datasets would provide ground truth data for videos, so it would be possible to compare when certain pedestrians were found with when they actually appeared. Datasets providing ground truth images of pedestrians could be useful for training the classifier, giving it examples of how pedestrians may appear in the footage. Different datasets were used to ensure the pedestrian detection is robust by applying it to various environments.

The CAVIAR project provides video clips featuring actors in common scenarios of interest for CCTV cameras. These include clips of people entering and leaving shops, meandering outside shops, people running etc. These videos also contain shadows, various lighting effects and reflections, so it would be ideal for testing and developing the pedestrian detector. CAVIAR also provides ground truth files for each of the videos which will be useful for analysing the performance of the program [8].

CVLAB multi-camera sequences of pedestrian behaviours for developing people detection algorithms and frameworks. This dataset contains video files with different angles of a pavement area with little to no shadows or reflections. These videos are useful for testing and demonstrating the program in a cleaner environment with less lighting interference [9].

The Daimler pedestrian segmentation benchmark provides contour-labelled and ground truth outlines of pedestrian shapes taken with a stereo camera. The ground truth images provided in this dataset could be useful for training the classifier. It provides a variety of formats for pedestrians including source images, contour outlines and binary ground truth shapes [10].

OpenCV is an open source computer vision library that is optimised for C++ programming. OpenCV provides a wide range of implementations for feature selection methods such as Haar, as well as basic image processing/video reading functions that would be useful for the project.

The ‘Mat’ class is OpenCV’s basic image container used for reading and writing images. It is a matrix containing pixel intensities that come in various formats such as greyscale (0-255) and blue/red/green (BGR). Mat’s memory is also automatically allocated, even when passing on existing Mat objects. This class can be used in the program for reading frames from video footage so they can be processed later, as well as loading dataset images for training purposes [11].

OpenCV has a ‘VideoCapture’ class that outputs frames from a video into a Mat object. The VideoCapture class allows videos to be played in real time by iterating over the frames while displaying each one. This would be useful for getting live feedback from not only the source footage but any analysis the program can give.

### Motion Detection Choice

For pedestrian detection, the people that appear in the footage will be always moving in and out of the scene, so it makes sense to have a motion based system. Having a system that prioritises movement will help filter hours of inactive scenes that occur in security footage backlogs. This also means that the motion detection must be reliable, as a low sensitive motion detector may miss key moments that occur during the video. Having an appropriately tuned motion detector ensures that the pedestrian detection can be reliable and precise.

As discussed in 1.1.4., BGS excels at highlighting moving objects from static perspectives such as a CCTV camera. In a still environment such as an alleyway or corridor, pedestrians moving in the scene are highly noticeable, especially in BGS. While optical flow helps represent large areas of motion, it would be more sensitive than BGS in an environment such as these. Optical flow could be considered overkill for such static environments, and may even perform worse depending on the quality of the cameras used. Using BGS reduces the complexity of the project, as it outputs binary images. This makes processing and representing pedestrian shapes easier.

OpenCV provides several implementations of BGS, with some flexibility to the thresholds used. Allowing the user to input the threshold values allows them to tune the pedestrian detection to suit the video’s scene. Some environments require different levels of history, depending how fast the pedestrians move within the scene. The BGS view can be displayed alongside the source video files, so the user can see what areas of the image are being processed.

### Feature Selection and Classification

Although BGS provides an adequate solution to detecting moving areas of interest, it doesn’t interpret what it’s looking at like Haar/HOG does. It’s important for programs such as these to not only detect, but to draw conclusions from the data it’s given. By combining BGS with feature selection, the program can use basic classification to distinguish between people and noise.

OpenCV provides an implementation for the Haar cascade classifier, which was implemented to test how well it performed on one of the CAVIAR videos. Despite trying out various minimum/maximum ranges for the object sizes, the ‘detectMultiScale’ function had a slow performance along with many false positives. Instead of using the Haar algorithm, an alternative approach was taken involving localised feature detection combined with BGS. BGS can be used to extract shapes from the source footage that may appear as pedestrians, and by locating features within certain areas of the shape, a larger skeleton model can be derived.

This skeleton model attempts to locate human features such as the head, hands and feet within the shape. The regions that each feature appears in can be taught through the training phase, where the code fits the feature skeleton to examples of pedestrians in BGS. Ground truth binary images such as those in the Daimler dataset have a similar appearance to shapes within BGS, so they are useful for the training stage. Once training is finished, the code will know which areas of the shape the features should appear. When running the skeleton finder on the video shapes, features located outside these regions will be considered invalid. The classifier can then count the number of features in the model that are valid, models with a certain number of valid features will be considered pedestrians and recorded within the log.

### Record Log

Choices for storing the record log data came down to using a table within a HTML/Excel file or using a database. A database would be unnecessary for this project as it would bring redundant functionality. If this project was installed on a high security system, having a database with restricted access would be useful for protecting pedestrian logs from being edited by unauthorised personnel. Writing code to output information to Excel format may be difficult, whereas HTML table tags are an easier alternative and can also be viewed on a wider variety of formats.

### Issues

Computer vision systems often rely on assumptions, which can either be based on logic or predications. Examples of logic assumptions include the ways that the skeleton model looks for features. It assumes that the head will always appear towards the top of the shape with shoulders just below, and that feet would appear below the waist. A prediction assumption would be that the pedestrians are always walking in the videos, when they may stop to stretch or sit down. These assumptions could lead the system to struggle with particular pedestrian poses.

A big assumption is that pedestrian shapes will be isolated, when more complex environments will have groups of pedestrians passing by each other. Since BGS relies on binary images, it will have less information for breaking down occluding shapes. The system will need to handle different orientations for people, most environments will have people in different directions. Also need to consider how such a system can deal with lighting, shadows and reflections, as they could distort the appearance of the shape.

Not only will variations in orientations occur, there will be variations in pedestrian appearance such as their clothing, skin tone and size. Environments such as military bases and offices will have uniform clothing, public areas however would have greater variations in appearance. Also need to consider pedestrians with holding items, objects such as bags, rucksacks and equipment could potentially distort the binary shapes.

One way to judge the performance of the pedestrian detector is by looking at the rate of false positives and negatives. False negatives could be argued as a bigger issue, pedestrian detection that believes no one is there when a trespasser is present could be detrimental to a security system. Efforts to reduce false positives should be considered, if the detector is consistently finding pedestrians when they are not present, users may lose trust in the system.

BGS will often pick up traces of small areas of motion, it is important to consider techniques for filtering smaller sizes of motion as they most likely not be pedestrians (thus reducing the false positive rate). Most cameras will contain noise due to resolution and speckle effects, so it’s important to consider noise reduction implementations.

### Security

With a project related to surveillance, it’s important to consider the security aspects and ethics of the work being done. The chosen datasets allow the videos and images to be used for academic purposes, and the actors within the videos are aware that they’re being recorded. No video sources have been used where pedestrians are unaware that they are being filmed. Websites hosting 24 hours livestreaming were avoided for this reason. Any videos recorded by myself were done ensuring that the people within the videos gave consent to record them.

It’s also vital to ensure no copyrighted material has been downloaded and played back through the program. Websites such as YouTube were avoided as it can be difficult to verify the uploader of the video and ensure that they’ve taken the correct precautions with their footage. Videos involving areas of restricted access were avoided, having pedestrian logs of high risk areas is forbidden.

## Process

### Methodology

For the software development side of the project, taking an agile approach allows the project to evolve and adapt throughout the development process. With a topic such as computer vision, goals and tasks are likely to change as algorithms are tested on dataset videos. Issues may arise that may contradict the goals originally set. A sequential model such as waterfall could restrict the necessary changes needed to increase the efficiency of the program.

Feature Driven Development (FDD) is a form of agile software development, it is a model-driven iterative process where the goals are defined by the necessary features. FDD involves having idea of the overall model and having a general idea of what features will be needed. Having a features list provides clear concise goals, while allowing necessities discovered during implementation to be included. FDD also has more flexible working hours than other methodologies such as Scrum which rely on sprints. Since this is a one-man project, other methodologies such as Extreme Programming that rely on pair programming aren’t as applicable. This also means that parts of FDD must be modified, such as generalising the team roles.

### Support tools

There are many IDE’s to support C++ development, IDE’s are useful as they highlight common errors in code and simplify the compilation process. Visual Studio 2015 proved useful for the project, as integrating the OpenCV framework into the project was quick and easy. The structure of the code could be easily managed using the project managers and class view tabs.

The project was stored in a git repository via BitBucket, a web service for hosting source code for large scale projects. Backing up code using a web-hosting service is more reliable and efficient than exporting it to USB, especially for larger projects. Documentation could also be exported to git, which made it easier to work on it from multiple machines. A diary was kept throughout development to keep track of the progress made as well as any sources or useful websites.

# Design

## Overall Architecture




Fig 5. Flow of information with the overall model

As you can see from Fig 5, an overall model of the system was drafted displaying the relationships between the core functionality. The people finder assumes that it will be looking at outlines of binary image shapes. Before the program runs the video, the blob detector outlines contours for the images so the people finder can be trained on the same format. Once the people finder has finished training, the video loop begins playing the video while applying BGS. The video loop is needed to iterate through each frame in the source video. Background subtraction can then be used to find moving objects in the video, as it has knowledge of the previous frame in the loop. The blob detector will then draw contours around the shapes, and outline the larger shapes that could potentially be pedestrians. A list of shapes is returned to the video loop so they can be displayed and used in the record log. The people finder applies the skeleton building function on the shapes, and determines whether the shape is a pedestrian or not. The people finder’s interpretations of the shapes and verdicts are returned to the video loop so they can be recorded in the log.

The video loop helps encapsulate information between the different parts of the program so they it can be summarised in the record log. Having each class create their own versions of the log could convolute it. BGS may also need to be integrated into the video loop, as keeping the BGS separate from the frames could interfere with the motion detection.

Other ways this design is better than alternatives. False positives with classification

## Features List and feature design plans

After developing an overall model of the program, a list of features was created to formalise the requirements to be completed. Each feature describes a necessary action that may be done multiple times throughout the program. Plans were also created for each feature which describes how they work. A summary of the features can be seen below:

* Input threshold values and paths into a menu
* Loading the training data
* Outlining shape contours
* Building the pedestrian models\*
* Training the pedestrian finder
* Running the input video
* Applying BGS
* Classifying shapes
* Record findings

The pedestrian model requires more detail through sub features, listed below:

* Searching for the head
* Torso
* Waist
* Feet
* Shoulders
* Elbows
* Hands
* Drawing the feature skeleton

### Input threshold values and paths into a menu

When the program loads, it presents the user with a menu where they can enter the training folder path, video path and BGS thresholds. A user interface is unnecessary as long as the user is able to input values and have the program filter invalid responses.

### Loading the training data

A directory path is entered from the input menu of the program, this path leads to a folder containing the images that the people finder will be trained on. The code retrieves the paths for each file. Using OpenCV’s image handling, each image is loaded using the paths.



Fig 6. Binary images of pedestrians from the Daimler dataset [10]

### Outlining shape contours




Fig 7. Flow chart for outlining shape contours.

Outlining shape contours is needed for training and testing. Input images for testing are resized and outlined so the people finder has a better idea of where the shape boundaries are. It is used during the video stage to extract the larger moving shapes within the overall frame. It assumes that the input images it receives are in binary format. Resizing shapes to the same size makes it easier for the people finder to interpret them.

### Building the pedestrian models




Fig 8. Summary of the detection process using CVLAB’s dataset [9]. Left to right: Source video, BGS, contour outline, pedestrian skeleton model

As with the shape contours, building pedestrian models will have similar functionality when being used for non-trained and trained examples. The main people finder class calls each of the local feature finding function to fit a pedestrian model to the shape. After locating the pedestrian features it plots them within the contour outline and connects the corresponding body parts. The sub features for this process are discussed in 2.3.

### Training the pedestrian finder




Fig 9. An example of the minimum and maximum boundary that valid head features fall within (green square) using the Daimler dataset [10].

As the people finder applies pedestrian models to the training images, it takes the minimum and maximum (x, y) positions for each feature. This creates rectangular regions which features from the video shapes must appear within to count as a valid feature. After the people finder is trained, it can differentiate between pedestrians and noise using these position ranges.

### Running the input video

With the help of OpenCV, the video is loaded and a frame is opened each loop iteration. These frames are displayed in windows, with the windows being updated with each new frame. As long as the performance is optimal the videos run smoothly on the screen. The BGS version of the frame will be visible alongside the source video as well as the outlined shapes.

### Applying BGS

For each new frame, OpenCV’s BGS function is applied. The binary image created using the function is filtered to reduce the noise. Optimal methods of filtering involved using a closing operation (dilation then erosion) followed by an opening operation (erosion then dilation) to reduce the speckle noise produced in the videos (**see section 3/4).** Dilation is the opposite of erosion in that it looks to expand areas with low pixel values within the kernel. These binary images are sent to the blob detector so the larger shapes can be extracted.

### Classifying shapes




Fig 10. Flow chart of the classification process

The people finder classifies the skeleton model built within the current shape. The program uses a feature tally system to decide whether the shape is a pedestrian. The feature skeleton consists of ten (x, y) coordinates that represent the different parts of the pedestrian. Each feature has their own (x, y) boundaries that were set during the training phase. Using the head feature for example, if the head feature plotted in the current shape falls within the boundaries, the feature is considered valid and the score increases. This is done for every feature, the resulting score determines what the verdict for the shape will be.

### Record findings




Fig 11. Example of the record log produced by the program that’s running a CVLAB video [9]

A new HTML file is created before running the video. The settings and directories used during runtime are saved, and the table is initialised. After classifying all the shapes found in the current frame, the log creates a new record for each one. The frame number and the timestamp indicate when the shape was found, along with the source of the shape and how the pedestrian detector interpreted it.

## Pedestrian model sub features

IMAGE OF PEDESTRIAN SKELETONS

### Search for the head

## Final classes

### Data Structures

### Method Allocation

You should concentrate on the more important aspects of the design. It is essential that an overview is presented before going into detail. As well as describing the design adopted it must also explain what other designs were considered and why they were rejected.

The design should describe what you expected to do, and might also explain areas that you had to revise after some investigation.

Typically, for an object-oriented design, the discussion will focus on the choice of objects and classes and the allocation of methods to classes. The use made of reusable components should be described and their source referenced. Particularly important decisions concerning data structures usually affect the architecture of a system and so should be described here.

How much material you include on detailed design and implementation will depend very much on the nature of the project. It should not be padded out. Think about the significant aspects of your system. For example, describe the design of the user interface if it is a critical aspect of your system, or provide detail about methods and data structures that are not trivial. Do not spend time on long lists of trivial items and repetitive descriptions. If in doubt about what is appropriate, speak to your supervisor.

You should also identify any support tools that you used. You should discuss your choice of implementation tools - programming language, compilers, database management system, program development environment, etc.

Some example sub-sections may be as follows, but the specific sections are for you to define.

Section: Overall model Flow/Flow of control chart. Small class UML/class diagrams at the end?. Section: FDD FEATURES LIST, FIVE STAGES

Include a diagram of Source->BGS->Contours->Shape/Skeleton

Section: each feature plan design. TALK ABOUT WHAT THE FEATURE DOES INCLUDE OPENCV STUFF AS FEATURES, SMALL FLOW CHARTS.

AN ALTERNATIVE APPROACH WAS.

2.2 FEATURES LIST = PLAN TALK, 2.4 FULL MONTY CODE TALK.

OpenCV’s BGSKNN BGSMOG. OpenCVs BGS equation(design?) Ask supervisor: do parts of my analysis fall under design, timeline Visio projessional.

Split up localised features into sections, pseudocode the algorithms (Not at mathematic level just yet).

# Implementation

The implementation should look at any issues you encountered as you tried to implement your design. During the work, you might have found that elements of your design were unnecessary or overly complex; perhaps third party libraries were available that simplified some of the functions that you intended to implement. If things were easier in some areas, then how did you adapt your project to take account of your findings?

It is more likely that things were more complex than you first thought. In particular, were there any problems or difficulties that you found during implementation that you had to address? Did such problems simply delay you or were they more significant?

You can conclude this section by reviewing the end of the implementation stage against the planned requirements. Code? Nodes vector for features helps keep it together (providing index numbers remembered). ISSUES AND PROBLEMS. Negative training examples unnecessary. Apply pedestrian detection every second instead of every frame.

# Testing

Detailed descriptions of every test case are definitely not what is required here. What is important is to show that you adopted a sensible strategy that was, in principle, capable of testing the system adequately even if you did not have the time to test the system fully.

Provide information in the body of your report and the appendix to explain the testing that has been performed. How does this testing address the requirements and design for the project?

How comprehensive is the testing within the constraints of the project? Are you testing the normal working behaviour? Are you testing the exceptional behaviour, e.g. error conditions? Are you testing security issues if they are relevant for your project?

Have you tested your system on “real users”? For example, if your system is supposed to solve a problem for a business, then it would be appropriate to present your approach to involve the users in the testing process and to record the results that you obtained. Depending on the level of detail, it is likely that you would put any detailed results in an appendix.

The following sections indicate some areas you might include. Other sections may be more appropriate to your project. BGS TESTING SECTION 2.2.6. EROSION DILATION OPTIMAL.

## Overall Approach to Testing

## Automated Testing

### Unit Tests

### User Interface Testing

### Stress Testing

### Other Types of Testing

## Integration Testing

## User Testing

# Critical Evaluation

Examiners expect to find in your dissertation a section addressing such questions as:

* Were the requirements correctly identified?
* Were the design decisions correct?
* Could a more suitable set of tools have been chosen?
* How well did the software meet the needs of those who were expecting to use it?
* How well were any other project aims achieved?
* If you were starting again, what would you do differently?

Other questions can be addressed as appropriate for a project.

Such material is regarded as an important part of the dissertation; it should demonstrate that you are capable not only of carrying out a piece of work but also of thinking critically about how you did it and how you might have done it better. This is seen as an important part of an honours degree. Can handle orientations

There will be good things and room for improvement with any project. As you write this section, identify and discuss the parts of the work that went well and also consider ways in which the work could be improved.

In the latter stages of the module, we will discuss the evaluation. That will probably be around week 9, although that differs each year.

# Appendices

The appendices are for additional content that is useful to support the discussion in the report. It is material that is not necessarily needed in the body of the report, but its inclusion in the appendices makes it easy to access.

For example, if you have developed a Design Specification document as part of a plan-driven approach for the project, then it would be appropriate to include that document as an appendix. In the body of your report you would highlight the most interesting aspects of the design, referring your reader to the full specification for further detail.

If you have taken an agile approach to developing the project, then you may be less likely to have developed a full requirements specification. Perhaps you use stories to keep track of the functionality and the ’future conversations’. It might not be relevant to include all of those in the body of your report. Instead, you might include those in an appendix.

There is a balance to be struck between what is relevant to include in the body of your report and whether additional supporting evidence is appropriate in the appendices. Speak to your supervisor or the module coordinator if you have questions about this. GITHUB LINK DIARY LINK. Microsoft windows library https://www.draw.io/

* 1. Third-Party Code and Libraries

If you have made use of any third party code or software libraries, i.e. any code that you have not designed and written yourself, then you must include this appendix.

As has been said in lectures, it is acceptable and likely that you will make use of third-party code and software libraries. If third party code or libraries are used, your work will build on that to produce notable new work. The key requirement is that we understand what is your original work and what work is based on that of other people.

Therefore, you need to clearly state what you have used and where the original material can be found. Also, if you have made any changes to the original versions, you must explain what you have changed.

As an example, you might include a definition such as:

**Apache POI library** – The project has been used to read and write Microsoft Excel files (XLS) as part of the interaction with the client’s existing system for processing data. Version 3.10-FINAL was used. The library is open source and it is available from the Apache Software Foundation [5]. The library is released using the Apache License [6]. This library was used without modification.

* 1. Ethics Submission

This appendix includes a copy of the ethics submission for the project. After you have completed your Ethics submission, you will receive a PDF with a summary of the comments. That document should be embedded in this report, either as images, an embedded PDF or as copied text. The content should also include the Ethics Application Number that you receive.

* 1. Code Samples

This is an example appendix. Include as many appendices as you need. The appendices do not count towards the overall word count for the report.

For some projects, it might be relevant to include some code extracts in an appendix. You are not expected to put all of your code here - the correct place for all of your code is in the technical submission that is made in addition to the Final Report. However, if there are some notable aspects of the code that you discuss, including that in an appendix might be useful to make it easier for your readers to access.

As a general guide, if you are discussing short extracts of code then you are advised to include such code in the body of the report. If there is a longer extract that is relevant, then you might include it as shown in the following section.

Only include code in the appendix if that code is discussed and referred to in the body of the report.

Random Number Generator

The Bayes Durham Shuffle ensures that the pseudo random numbers used in the simulation are further shuffled, ensuring minimal correlation between subsequent random outputs.

// Some example code here…

# Annotated Bibliography

This final section should list all relevant resources that you have consulted in researching your project. Each reference should also include a brief annotation.

1. John Perdikaris, “*Physical Security and Environmental Protection*”, January 2014, Chapter 5.3 Surveillance and Counter Surveillance, page 147.
2. UK Government, “*Plug and Play Autonomous Sensors*”, 2015. Available: <https://www.gov.uk/government/news/plug-and-play-autonomous-sensors>. [Accessed 06 February 2017].

A press release discussing the development of new concepts in modular autonomous sensing. Provides details on some of the technologies used.

1. Gavin J.D Smith, “*Behind the Screens: Examining Constructions of Deviance and Informal Practices among CCTV Control Room Operators in the UK*”, pages 388-389, 2004. Available: <http://surveillance-and-society.org/articles2(2)/screens.pdf>. [Accessed 18 April 2017].
2. BBC, "*Missing Corrie Mckeague: Suffolk Police ‘search lacks resources’”,* November 2016. Available: <http://www.bbc.co.uk/news/uk-england-suffolk-38052508>. [Accessed 18 April 2017]
3. Paul Viola & Michael J. Jones, “*Robust Real Time Face Detection”,* received September 2001, pages 138-139. Available: <http://www.vision.caltech.edu/html-files/EE148-2005-Spring/pprs/viola04ijcv.pdf>. [Accessed 19 April 2017]
4. Shanshan Zhang, Christian Bauckhage, Armin B. Cremers, “*Informed Haar-like Features Improve Pedestrian Detection*”, 2014 IEEE Conference on Computer Vision and Pattern Recognition, pages 949-950.
5. Navneet Dalal & Bill Triggs, “*Histograms of Oriented Gradients for Human Detection*”, 2005 IEEE Computer Society Conference on Computer Vision and Pattern Recognition (CVPR’05), Chapters 3 & 6.4.
6. EC Funded CAVIAR project/IST 2001 37540, found at URL: [*http://homepages.inf.ed.ac.uk/rbf/CAVIAR/*](http://homepages.inf.ed.ac.uk/rbf/CAVIAR/). [Accessed 20 April 2017]

Dataset containing video footage for testing/demonstrating the project.

#### [9] Jérôme Berclaz, François Fleuret, Engin Türetken, Pascal Fua “Multiple Object Tracking using K-Shortest Paths Optimization” IEEE Transactions on Pattern Analysis and Machine Intelligence 2011

CVLab – EPFL. “*Multi-Camera pedestrian videos*”, available at: <http://cvlab.epfl.ch/data/pom>. [Accessed 20 April 2017]

[10] F. Flohr and D. M. Gavrila.   
*“PedCut: an iterative framework for pedestrian segmentation combining shape models and multiple data cues.”* Proc. of the British Machine Vision Conference, Bristol, UK, 2013.

Daimler dataset, available: <http://www.gavrila.net/Datasets/Daimler_Pedestrian_Benchmark_D/Daimler_Pedestrian_Segmentatio/daimler_pedestrian_segmentatio.html> [Accessed 20 April 2017]

[11] OpenCV, “*Open source computer vision and machine learning software library*”, available: <http://opencv.org/> [Accessed 24 April 2017]